# Functions Which Can Be Specified from the Control Panel

This printer allows you to specify the printing functions from the printer driver. However, some printing functions are specified from the control panel or the Remote UI. The following table shows the functions to be specified from the control panel or the Remote UI.
For details on the items you can manage using the control panel, see "Setting Items."

Function | Overview of the Function
Multi-purpose tray paper size | Specifies the size of the paper loaded in the multi-purpose tray. "[Setup] Menu ([Paper Source] Options)" "[Select Feeder] Menu"
Multi-purpose tray priority | Specifies whether the printer should detect the paper source in order starting with the multi-purpose tray. "[Setup] Menu ([Paper Source] Options)"
Drawer N (N = 1, 2) size | Specifies the size of the paper loaded in the drawer (Drawer 1 or 2). "[Setup] Menu ([Paper Source] Options)" "[Select Feeder] Menu"
Standard paper size | Since paper size cannot be specified when printing from DOS, UNIX or other operating system, specify it using this setting. "[Setup] Menu ([Paper Source] Options)"
Invalid paper tray | Specifies what the printer does when paper that is the same size as the paper size of the received data is not loaded in the selected paper source. "[Setup] Menu ([Paper Source] Options)"
Auto selection | Specifies the paper source to be automatically selected. "[Setup] Menu ([Paper Source] Options)"
Standard paper type | Since paper type cannot be specified when printing from DOS, UNIX or other operating system, specify it using this setting. "[Setup] Menu ([Paper Source] Options)"
Alternative method | If the last page for the 2-sided printing is 1-sided printing, 1-sided printing is applied to the last page. "[Setup] Menu ([Layout] Options)"
Advanced Smoothing | Set whether to use the smoothing process to print the jagged edges of text and graphics. "[Setup] Menu ([Quality] Options)"
Recovery printing | Specifies whether to print the partially printed page when the printer stops printing due to a paper jam or an error occurring. "[Setup] Menu ([User Maintenance] Options)"
Check paper size | Specifies whether the printer should stop printing, displaying the message <Check paper size.> or continue printing. "[Setup] Menu ([User Maintenance] Options)"
Substitute size | The printer switches the paper size if the paper of the size to be used is not loaded in the printer. "[Setup] Menu ([User Maintenance] Options)"
Plain paper curl adjustment | If printed plain paper curls, specify the setting for this item. "[Setup] Menu ([User Maintenance] Options)"

0258-060