# The Printer Takes a Long Time to Start the Print Job

Perform one of the following solutions according to the cause.

#### <Cause 1> The printer is cooling down to maintain print quality. (Especially after narrow paper is printed)

Solution | Wait a moment. The printer automatically cools down the inside. After cooling is completed, the printer resumes printing.

#### <Cause 2> This problem may occur in some applications depending on the processing type of the print data. (Windows 2000/XP/Server 2003)

Solution | If you are using the PCL/UFR II printer driver, performing the following procedure may be able to solve the problem. UFR II Printer Driver
1. | Display the [Finishing] sheet.
2. | Click [Advanced Settings].
3. | Change the [EMF Spooling] setting.
PCL Printer Driver See Help of the PCL printer driver.

0258-0AK