# Checking the SD Card Installation

After installing an SD card, print Configuration Page to check if the module is installed properly.

NOTE
###### Load A4 size paper. Configuration Page is designed to be printed on A4 size paper. Be sure to load A4 size paper when printing the Configuration Page.

1
Load A4 size paper in the multi-purpose tray or drawer.
"Paper Loading and Output"
2
Make sure that the printer is online.
If the printer is not online, press [ ] (: Online).
3
Press [ ] (: Utility).
4
Select [Configuration Page] using [ ] and [ ], and then press [OK].
5
Select [Yes] using [ ], and then press [OK] to print Configuration Page.

NOTE
###### How to check the installation Check to make sure that [SD Card] under the [Control Menu] is set to [On].
→ | If [SD Card] is not displayed, see "Removing SD Card" and remove the SD card once.
→ | If the [SD Card] is [Off], set it to [On] using the following procedure.
(1) | Press [ ] (: Settings).
(2) | Select [Control Menu] using [ ] and [ ], and then press [OK].
(3) | Select [SD Card] using [ ] and [ ], and then press [OK].
(4) | Select [On] using [ ] and [ ], and then press [OK].
(5) | Hard reset or restart the printer.
→ | Check that the SD card is not write-protected. If the card is write-protected, release the protection, and then insert the card.
| The above figure is a sample of Configuration Page. The contents may differ from the Configuration Page printed by your printer.

0258-0RW