# Clearing Paper Jams (Back Cover)

Referring to the procedure on the display, follow the steps below to remove jammed documents.
1
Press [ ].
2
Open the back cover.
3
Open the paper output guide by holding the green tab (A).
4
Remove the paper by pulling it gently.
Make sure that no paper is jammed inside the paper output guide, and then close it.
5
Remove the paper by pulling it gently.
6
Holding the tabs (A) on both sides, close the 2-sided unit.
Close the guide firmly until it clicks.
7
Remove the paper by pulling it gently.
8
Close the rear cover.
The machine is ready to print.

Next, proceed to the clearing procedure for another area which is displayed in the message.
| (1) "Clearing Paper Jams (Multi-purpose Tray)"
| (2) "Clearing Paper Jams (Paper Drawer)"
| (3) "Clearing Paper Jams (Back Cover)"
| (4) "Clearing Paper Jams (Output Area)"

0258-0C6