# Control Panel Setting

This section describes the menu operation for this printer.

## Procedure for the Menu Operation

The menu consists of three hierarchies: "Option", "Item", and "Setting Value." Select the target options in each hierarchy.
As an example of the setting procedure, this section describes the procedure for setting [Gradation Level] in the [Quality] options to [High]. Start the key operation from Step 1.

Before specifying the setting, see "Attention (Control Panel Setting)."

| ###### Operation Procedure | Key Operation
1 | Place the printer offline. | Press [ ] (: Online).
When the printer is online, the [Setup] menu can be displayed, however, the [User Maintenance] options cannot be specified.
2 | Display the [Setup] menu. | Press [ ] (: Settings).
The [Setup] menu is displayed.
3 | Select the option. When the [Quality] options are selected | Press [ ] or [ ].
The target option is displayed.
4 | Display the item. | Press [OK].
The selected item is displayed.
5 | Select the item. When [Gradation Level] is selected | Press [ ] or [ ].
The target item is displayed.
6 | Select the item. | Press [OK].
The selected setting value is displayed.
7 | Select the setting value. When [High 2] is selected | Press [ ] or [ ].
The target setting value is displayed.
8 | Determine the selected setting value. | Press [OK].
The target setting value is specified. The setting completion screen is displayed for 3 seconds. You can change the display time for the screen using [Set. Comp. Notify] in the [Setup] menu.
9 | Go out of the setting menu. | Press [ ] (: Online).

## Printer Status to Enter the Menu Operation

You can enter each menu when the printer is in the following status.
: The state where you can enter the menu
: The state where you cannot enter the menu

| When the printer is ready to print *1 | When an error is occurring *2
When the printer is online | When the printer is offline
[Setup] Menu | *3 |  |
[Select Feeder] Menu |  |  |
[Reset] Menu |  |  | *4
[Job] Menu |  |  |
[Utility Menu] Menu |  |  |

*1 | The printer is ready to print when the Ready indicator is on.
*2 | An error is occurring in the printer when the Message indicator is on.
*3 | The [User Maintenance] options cannot be specified.
*4 | You cannot perform [Form Feed].

0258-08H