# Printing on Transparencies (B&W Printing Only)

#### Confirming usable transparencies

This printer can use the following sizes of transparencies.

Standard sizes | A4, Letter

Transparencies can only be printed in B&W.

#### Loading transparencies

You can load transparencies only in the multi-purpose tray.
"Loading Paper in the Multi-purpose Tray"

###### <Precautions when loading transparencies>

Thoroughly fan the transparencies, and then align the edges before loading them as they may stick to each other. If they are not fanned enough, multiple sheets of paper may be fed at once, causing paper jams.
When fanning or aligning the transparencies, try to hold the edges to avoid touching the printing surface.
Take care not to mark or stain the printing surface of the transparencies with fingerprints, dust, or oil. This may result in poor print quality.

#### Printing from an application

After loading transparencies, perform printing.
"Configuring the Printer Driver and Printing"

|  | The print speed drops when printing on transparencies.

0258-03Y