# Receiving and Printing E-mails Manually

IMPORTANT
###### Receiving E-mails The printer can receive e-mails only when it is online. ###### When using POP3 protocol When it is set to receive e-mail automatically using [POP3 RX Interval], if you attempt to receive e-mail manually while e-mail is being received automatically, your actions will be ignored. "How to Specify the Settings for E-mail Print" ###### When using SMTP protocol It automatically receives and prints e-mails. There is no need to manually receive and print them. "How to Specify the Settings for E-mail Print"

## Printing from the Printer Control Panel

1
Make sure that the printer is online.
If the printer is not online, press [ ] (: Online).
2
Press [ ] (: Utility) to display the Utility menu.
3
Press [] and [], select [E-Mail Print Utility], and then press [OK].
4
Press [] and [], select [Received E-Mails], and then press [OK].
5
When <Run?> is displayed, press [], select [Yes] and press [OK].
The printer is connected to the mail server. The printer receives e-mails addressed to the printer and print them.

## Printing from a Remote UI

1
Start the Remote UI.
"Starting the Remote UI"
2
Select [Network] under [Preferences] in the [Settings/Registration] menu.
3
Click [E-Mail RX] that is on the right side of [E-Mail Print Settings].
The printer is connected to the mail server. The printer receives e-mails addressed to the printer and print them.
0258-0FL