# Outputting Data (Forced Output)

When a job is canceled from the computer or the data is less than one page, the data may remain in the printer memory, and the job may not be completed properly. As long as the printer remains in this state, you cannot perform printing because the printer cannot receive the next data.
In this case, force the printer to output the print data using the following procedure.

IMPORTANT
###### If you cannot output data You cannot output data for the following jobs or in the following state. Data from the PCL/PS/UFR II printer driver The state where the Message indicator is on Perform a soft reset. "Canceling the Process Currently Being Performed (Soft Reset)"
###### The data that is being printed is deleted. When you output data, print it again.

NOTE
###### About automatic output When [Timeout] under [Interface] in the Setup Menu is set to [On], even less than a page worth of data is discharged automatically. (Data from the PCL/UFR II printer driver is not output.) [Timeout] for a job is set to 15 seconds in the default settings.

1
Press [ ] (: Reset).
2
Select [Form Feed] using [ ] and [ ], and then press [OK].
3
Select [Yes] using [ ], and then press [OK].

→ | The data remaining in the memory is printed.

IMPORTANT
###### If the Job indicator does not go off even after outputting the data Perform a soft reset. "Canceling the Process Currently Being Performed (Soft Reset)"

0258-03L