# Copy Specifications

Scan Resolution | Text/Photo 300 x 600 dpi Text/Photo (Quality), Photo, Text 600 x 600 dpi
Output Resolution | 600 x 600 dpi
Copy Ratio | 100% (Direct), 400% (Max), 200%, 129% STMT->LTR, 78% LGL->LTR, 64% LTR->STMT, 50%, 25% (Min)
Copy Speed *1 (Letter Plain Direct) | 42 cpm
Continuous Copying Capacity | Maximum 999 copies
First Copy Time (Letter) | Platen glass: 7.8 seconds or less Feeder: 9.6 seconds or less
*1 The copy speed on Letter size plain paper on one-side printing is measured during continuous copying. However, this varies depending on the use conditions and environment of the machine.

0Y01-0F6