# Specifying Previously Used Destinations

|  | You can select a destination from among the past three destinations. When you specify a previously used destination, the machine also sets the same scan settings such as density you used the last time you sent documents to that destination.

When <Restrict Resending from Log> is set to <On>, you cannot use this feature. Disabling Use of Previously Used Destinations Turning OFF the machine or setting <Restrict New Destinations> to <On> deletes the past destinations, and disables this feature. Limiting Available Destinations

When you specify a destination using this feature, any destinations that you have already specified are deleted.

1
Press and tap <Scan>.
When the logon screen appears, use the numeric keys to enter the user name and password. Then select the authentication server and press . Logging on to Authorized Send
2
Select <Destination> <Recall Set.>.
3
Select a destination.
When you transmit to multiple destinations, only the address specified for the first transmission is displayed in the log, but all the destinations are specified.
The selected destination and its scan settings are specified. You can also change the settings before sending.

###### To delete destinations (e-mail/I-Fax)

When you transmitted to multiple destinations, you can delete destinations as necessary.

1 | Select <Destination> <Confirm/Edit>.
2 | Select a destination you want to delete.
3 | Tap <Remove>. If you select Group Dial in step 2, <Number of Destinations: XX> is displayed. Tapping this item displays destinations registered in the group.
4 | Tap <Yes>.

##### If you want to easily and quickly delete destinations without displaying a list of destinations Before tapping <Destination> in step 1, you can tap / to toggle the destinations you specified. Display a destination you want to delete, and press .

LINKS
Sending Documents as E-Mails Directly from the Machine
Sending I-Faxes
Saving Documents Directly in Shared Folder/FTP Server
0Y01-068