# Scanner Specifications

Type | Color scanner
Maximum Scan Size | Platen glass: up to 8 1/2" x 14" (215.9 x 355.6 mm) Feeder: up to 8 1/2" x 14" (215.9 x 355.6 mm)
Scan Resolution | Optical resolution Platen glass: up to 600 x 600 dpi Feeder: up to 300 x 300 dpi Software interpolation resolution 9,600 x 9,600 dpi
Scan Speed *1 (Letter, 300 x 300 dpi) | Color: Approx. 7 seconds/sheet Black and White: Approx. 3 seconds/sheet
Driver | TWAIN WIA 2.0 (Windows Vista/7/8) ICA (Mac OS X 10.6.x or later)
*1 Speed of scanning via the platen glass. The communication time is not included.

0Y01-0F8