# How to Replace the Waste Toner Container

Read the precautions in Maintenance and Inspections and Consumables before replacing the waste toner container.
1
Open the front cover.
2
Open the left cover.
3
Remove the waster toner container together with the left cover.
Be careful not to tilt the container. Tilting the waster toner container will result in spilling of collected toner.
4
Remove the waste toner container from the protective case.
Do not disassemble or modify the waste toner container.
5
Install the new waste toner container and close the left cover.
6
Close the front cover.
101K-08X