# Utility Menu

| You can display the total number of printed pages and print internal system information. When you press () on the operation panel, the Utility menu is displayed. You can specify the settings described below when the machine is offline.

Check Counter Configuration Page Network Status Print Consmbl. Status Prt. IPSec Policy List Calibration PCL Utility PS Utility Cleaning |  | Control Condensation E-Mail Print Utility Printing Pos. Print Page Count List Counter Report Print MEAP Sys. Info Serial Number Consumables Info.

## Check Counter

You can check the total number of printed pages. Checking Total Number of Printed Pages

You can also check the counter value by selecting <Check Counter> in the Setup Menu as well as this item.

##### 101: Total 1

You can check the total number of pages printed.

(Display only)

##### 108: Total (B&W 1)

You can check the number of pages printed in black and white.

(Display only)

##### 113: Total (B&W/Sml)

You can check the number of pages printed in black and white.

(Display only)

##### 114:Total 1(2-Sided)

You can check the number of pages printed in 2-sided printing mode.

(Display only)

##### 123:Total(Full+1C/S)

You can check the number of pages printed in color (other than e-mail printing).

(Display only)

## Configuration Page

You can check the machine settings (Setup Menu) configured in the machine. You can also check other information including the amount of remaining toner, the number of printed pages, and the capacity of the memory (RAM) mounted on the machine. Configuration Page

## Network Status Print

Select to print a list of the settings (Network) about the network configured in the machine. You can also check the information about the security including the address filter settings and IPSec settings. Network Status Print

## Consmbl. Status Prt.

The information such as toner remaining amount, warning messages, and information on where you can purchase new toner cartridges is printed out. Consmbl. Status Prt.

## IPSec Policy List

Select to print a list of the IPSec policy names and settings (Configuring IPSec Settings) configured in the machine. IPSec Policy List

## Calibration

When color mismatch occurs or when the colors have changed and the data is not printed in the correct colors (specified colors), you can perform calibration. Correcting Color Mismatch and Hues

##### Color Mismatch Corr.

Print color mismatch refers to a shift in the positions of colors that may occur when printing one image with multiple toner cartridges. When color mismatch occurs, correction can be made by adjusting the print start positions of the respective colors

##### Density Control

When the colors have changed and the data is not printed in the correct colors (specified colors), correction can be made by density control for the respective colors.

##### Full Calibration

Performs both <Color Mismatch Corr.> and <Density Control> simultaneously.

## PCL Utility

Select to print a list of the internal information items registered in the machine for use of the PCL mode.

##### Font List

Select to print a list of the fonts that can be used in the PCL mode. PCL Font List

## PS Utility

Select to print a list of the settings for use of the PS mode and the internal information items registered in the machine. PS Mode List

##### Configuration Page

Select to print a list of the machine settings (PS).

##### Font List

Select to print a list of the fonts that can be used in the PS mode.

## Cleaning

Select to clean the fixing unit when black spots or streaks appear on printouts. Fixing Unit

## Control Condensation

If rapid temperature changes occur in the environment where the machine is installed, printed images or text may be lighter or smudged. In this case, executing this function may solve the problem. If the problems persist, execute the function repeatedly.
() <Control Condensation> <Yes>

## E-Mail Print Utility

Select to manually receive e-mails and print a log of received e-mails in list form.

##### Received E-Mail

Select to manually receive e-mails from the POP3 mail server and print them. Manually Receiving E-Mails

##### E-Mail RX Log List

Select to print a log consisting of subjects and received date/time of e-mails received in the machine in list form. E-Mail Print Log

## Printing Pos. Print

Select to print marks that indicate the current print position. Adjusting Print Position

## Page Count List

Select to print a report on the number of printed pages for each department when Department ID Management is enabled. Page Count List

## Counter Report

Prints an aggregate report of the number of pages printed for each counter. Counter Report

## Print MEAP Sys. Info

Select to print a list of information about MEAP applications installed in the machine and the MEAP system applications when the MEAP function is enabled. Print MEAP Sys. Info

## Serial Number

Select to display the serial number of the machine.
() <Serial Number>

## Consumables Info.

Select to display the information about such as the paper and toner cartridge.

##### Paper Information

Select to display the currently specified paper size and paper type, and the remaining paper level for each paper source. Checking Paper

##### Toner Cart. Model

Select to display the model number of the toner cartridge for the machine. Checking the Toner Cartridge Model

##### Remaining Toner

Select to display the amount of remaining toner. Checking the Amount of Remaining Toner

The displayed remaining toner level can be used only as a guide and may differ from the actual level.

##### Waste Toner cntnr.

You can display the model number of the waste toner container. Checking the Model Numbers of Waste Toner Container

##### Waste Toner Status

You can display the status of waste toner container. Checking the Status of Waste Toner Container
101K-063