# Paper

### Supported Paper Sizes

Paper sizes that can be loaded in the paper drawer, multi-purpose tray, or optional paper sources are listed below.
: Available : Unavailable

Paper Size | Drawer 1 | Drawer 2 to 4 (optional) | Multi-Purpose Tray | Automatic 2-Sided Printing *1
A4 (210.0 x 297.0 mm) |  |  |  |
B5 (182.0 x 257.0 mm) |  |  |  |
A5 *2 (148.0 x 210.0 mm) |  |  |  |
A6 (105.0 x 148.0 mm) |  |  |  |
Legal (LGL) (215.9 x 355.6 mm) |  |  |  |
Letter (LTR) (215.9 x 279.4 mm) |  |  |  |
Statement (STMT) (139.7 x 215.9 mm) |  |  |  |
Executive (EXEC) (184.1 x 266.7 mm) |  |  |  |
Foolscap (FLSC) (215.9 x 330.2 mm) |  |  |  |
16K (195.0 x 270.0 mm) |  |  |  |
Index Card (76.2 x 127.0 mm) |  |  |  |
Indian Legal (215.0 x 345.0 mm) |  |  |  |
Government Legal (203.0 x 330.0 mm) |  |  |  |
Government Letter (203.0 x 267.0 mm) |  |  |  |
Australia Foolscap (206.0 x 337.0 mm) |  |  |  |
Postcard (100.0 x 148.0 mm) |  |  |  |
Reply Postcard (148.0 x 200.0 mm) |  |  |  |
4 on 1 Postcard (200.0 x 296.0 mm) |  |  |  |
Envelope NAGAGATA 3 (120.0 x 235.0 mm) |  |  |  |
Envelope YOUGATANAGA 3 (Younaga 3) (235.0 x 120.0 mm) |  |  |  |
Envelope No. 10 (COM10) (104.7 x 241.3 mm) |  |  |  |
Envelope Monarch (98.4 x 190.5 mm) |  |  |  |
Envelope C5 (ISO-C5) (162.0 x 229.0 mm) |  |  |  |
Envelope DL (110.0 x 220.0 mm) |  |  |  |
Custom Paper Size | *3 | *4 | *5 | *6
*1 Automatic 2-sided printing is available without replacing paper. *2 Can be loaded in portrait orientation. Automatic 2-sided printing is only possible when the paper is loaded in landscape orientation. *3 The following sizes are available: When loaded in portrait orientation (only with the UFR II printer driver used): 148.0 to 215.9 mm, 148.0 to 215.9 mm When loaded in landscape orientation: 101.6 to 215.9 mm, 148.0 to 297.0 mm *4 The following sizes are available: When loaded in portrait orientation (only with the UFR II printer driver used): 148.0 to 215.9 mm, 148.0 to 215.9 mm When loaded in landscape orientation: 101.6 to 215.9 mm, 148.0 to 355.6 mm *5 The following sizes are available: When loaded in portrait orientation (only with the UFR II printer driver used): 127.0 to 215.9 mm, 127.0 to 215.9 mm When loaded in landscape orientation: 76.2 to 215.9 mm, 127.0 to 355.6 mm *6 The following sizes are available: 148.0 to 215.9 mm, 210.0 to 355.6 mm

The default setting of paper size is <A4>. Change the paper size setting when using a different size of paper. Specifying Paper Size and Type in the Paper Drawer Specifying Paper Size and Type in the Multi-Purpose Tray Some paper sizes may not be displayed depending on the printer driver. If the paper size that you want to use is not displayed, download the UFR II / UFRII LT V4 printer driver from the Canon website. If you cannot download, contact your local authorized Canon dealer or the Canon help line.

### Paper Type and Paper Source Capacity

Chlorine-free paper can be used with this machine.

Print quality may deteriorate depending on the paper type used. Each source capacity indicated in the following table is merely a guide, so it may be different from the actual capacity.

: Unavailable

Paper Type | Drawer | Multi-Purpose Tray
Plain paper *1*2 | 60 to 80 g/m² | 550 sheets *3 | 100 sheets
81 to 90 g/m² | 400 sheets | 80 sheets
Heavy paper | 91 to 105 g/m² *2 | 400 sheets | 80 sheets
106 to 128 g/m² *2 | 400 sheets | 80 sheets
129 to 163 g/m² *2 | 250 sheets | 50 sheets
164 to 216 g/m² |  | 30 sheets
Rough paper *2 | 60 to 105 g/m² | 400 sheets | 80 sheets
Labels | 100 sheets |
Postcard/Reply Postcard/4on1 Postcard *4 |  | 50 sheets
Envelope |  | 10 sheets
*1 Recycled paper is also available. *2 Automatic 2-sided printing is available without replacing paper. *3 The source capacity when paper of 80 g/m² is used. For paper of 64 g/m², up to 640 sheets can be loaded. *4 The inkjet printable postcard or reply postcard can not be used.

### Paper Type and Setting for the Machine

Loading Paper

### Printable Area

The shaded areas in the image below indicate the printable area of the document. For envelope, the top, bottom, left, and right margins are all 10 mm.
101K-07R