# Select Feeder Menu

| The settings about the paper source and the size of paper loaded in the machine are listed with short descriptions. When you press () on the operation panel, the Select Feeder menu is displayed. Default settings are marked with a dagger ().

##### Common settings The settings are the same as those for <Paper Source> in the Setup Menu. The settings specified here are also applied to the <Paper Source> settings. ##### Asterisks (*) Settings marked with an asterisk (*) are not displayed depending on other settings or whether an optional paper feeder is installed in the machine.

Paper Source MP Tray Paper Size Drawer N Paper Size (N=1, 2, 3, 4) Standard Paper Size MP Tray Priority MP Tray for Mix Ppr. Auto Select Drawer |  | Auto Detect Ppr Type Default Paper Type MP Tray Paper Type Drawer N Paper Type (N=1, 2, 3, 4) Manual 2-Sided (MP) 2-Sided Printing

## Paper Source

Select the paper source from which paper is fed. When you want to automatically change the paper source based on the paper size and paper type, select <Auto>.

Auto Multi-Purpose Tray Drawer 1 Drawer 2 * Drawer 3 * Drawer 4 *

() <Paper Source> Select the paper source

## MP Tray Paper Size

Specify the size of the paper that is loaded in the multi-purpose tray. Specifying Paper Size and Type in the Multi-Purpose Tray

A6 A5 A5R B5 A4 LTR LGL EXEC Free Size Custom Size Custom Size R Postcard Reply Postcard 4on1 Postcard Env. Nagagata3 Env. Younaga 3 Env. ISO-C5 Env. Monarch Env. No.10 Env. DL Index Card STMT FLSC 16K

## Drawer N Paper Size (N=1, 2, 3, 4) *

Set the size of paper loaded in the machine's paper drawer or optional paper feeder's paper drawer (Specifying Paper Size and Type in the Paper Drawer).

#### Machine's Paper Drawer

A6 A5 A5R B5 A4 LTR EXEC Free Size Custom Size Custom Size R STMT 16K

#### Paper Feeder's Paper Drawer

A6 A5 A5R B5 A4 LTR LGL EXEC Free Size Custom Size Custom Size R STMT FLSC 16K

## Standard Paper Size

You cannot perform paper size setting on a computer running an operating system or a mobile device that does not support any printer driver. If you want to print from such computer or mobile device, use this item to set the size of the paper to print on.

A6 A5 B5 A4 LTR LGL EXEC Postcard Reply Postcard 4on1 Postcard Env. Nagagata3 Env. Younaga 3 Env. ISO-C5 Env. Monarch Env. No.10 Env. DL Index Card STMT FLSC 16K

() <Standard Paper Size> Select the paper size

#### Selecting the paper size

Specify the setting according to the size of the paper to print on.

## MP Tray Priority

Select whether to prioritize paper feeding from the multi-purpose tray when <Paper Source> is set to <Auto>. If you select <On>, paper is fed from the multi-purpose tray when the same size paper is loaded in both the multi-purpose tray and the paper drawer.

Off On

() <MP Tray Priority> <Off> or <On>

When <MP Tray for Mix Ppr.> is set to <On>, paper is preferentially fed from the paper drawer even if <MP Tray Priority> is set to <On>.

## MP Tray for Mix Ppr.

If you select <On> with <Paper Source> set to <Auto>, the multi-purpose tray is automatically selected when appropriate size paper is not loaded in any paper drawer.

Off On

() <MP Tray for Mix Ppr.> <Off> or <On>

## Auto Select Drawer

If you select <Use> with <Paper Source> set to <Auto>, the machine automatically selects the paper source with appropriate size paper loaded. Also, when the paper runs out, this setting enables continuous printing by switching from one paper source to another that is loaded with the same paper size.

Do Not Use Use

() <Auto Select Drawer> Select the paper source <Do Not Use> or <Use>

#### Paper source selection

Select the paper source to which you want to apply the Auto Select Drawer function.

#### Switching of the settings

Select <On> to enable automatic drawer selection for the paper source you selected on the previous screen ().

## Auto Detect Ppr Type

Specify whether to automatically detect the paper type when plain paper or heavy paper is loaded. To use this function, set the paper type for the paper source to <Mixed Types>. Also, set [Paper Type] in the printer driver to [Printer Default].
Paper
MP Tray Paper Type
Drawer N Paper Type (N=1, 2, 3, 4)
Basic Printing Operations

Multi-Purpose Tray Do Not Use First Sheet Only Each Sheet Drawer 1 Do Not Use Use Drawer 2 * Do Not Use Use Drawer 3 * Do Not Use Use Drawer 4 * Do Not Use Use

() <Auto Detect Ppr Type> Check the message Select the paper source Select the setting value

#### Paper source selection

Select the paper source for which you want to make a setting concerning automatic paper type detection.

#### Switching of the settings (Multi-Purpose Tray)

When <First Sheet Only> is specified, paper type detection is performed for the first sheet only. When <Each Sheet> is specified, paper type detection is performed for each sheet as it is fed.

#### Switching of the settings (Drawer 1 to 4*)

When <Use> is specified, paper type detection is performed for the first sheet only.

When this function is enabled, the printing speed may be slower. When <Each Sheet> is specified, the printing speed will be slower. When this function is enabled, the machine may not be able to print properly. If the machine cannot print properly, set this function to <Do Not Use> and specify the paper type from the printer driver before trying printing again.

## Default Paper Type

You cannot perform paper type setting on a computer running an operating system or a mobile device that does not support any printer driver. If you want to print from such computer or mobile device, use this item to set the type of the paper to print on.

Plain Plain L Plain L2 Heavy 1 Heavy 2 Heavy 3 Heavy 4 Postcard Envelope Labels Rough 1 Rough 2

() <Default Paper Type> Select the paper type

#### Paper type selection

Specify the settings in the same way as the paper settings in the printer driver according to the paper type for printing. Loading Paper

## MP Tray Paper Type

Set the type of paper loaded in the multi-purpose tray. Specifying Paper Size and Type in the Multi-Purpose Tray

Plain Plain L Plain L2 Heavy 1 Heavy 2 Heavy 3 Heavy 4 Postcard Envelope Rough 1 Rough 2 Mixed Types

## Drawer N Paper Type (N=1, 2, 3, 4) *

Set the type of paper loaded in the paper drawer. Specifying Paper Size and Type in the Paper Drawer

Plain Plain L Plain L2 Heavy 1 Heavy 2 Heavy 3 Labels Rough 1 Rough 2 Mixed Types

## Manual 2-Sided (MP)

Select the side of paper to print on when you want to perform 2-sided printing manually from the multi-purpose tray.

1st Side 2nd Side

() <Manual 2-Sided (MP)> <1st Side> or <2nd Side>

#### <1st Side>

Select to print on the back side (the side to print first).

#### <2nd Side>

Select to print on the front side (the opposite of the side that is already printed).

## 2-Sided Printing

Select whether to print on both sides of paper.

Off On

() <2-Sided Printing> <Off> or <On>
101K-066