# Adjusting Print Density

If the resulting print is darker or lighter than expected, you can adjust the toner density for each CMYK color. You can make fine adjustment of the toner density by dividing the whole density range into three areas.

If <Toner Save> is set to <On>, you cannot use this adjustment function. Toner Save

1
Press ().
2
Use / to select <Print Quality>, and press .
3
Adjust the density.

1 | Select the color whose density you want to adjust, and press .
2 | Use / to adjust the density. Density adjustment Set a "+" value to increase the density. Set a "-" value to decrease the density.
3 | Press .

###### Making fine adjustment of toner density by density level

You can make fine adjustment of toner density on three density levels - high, medium, and low.

1 | Use / to select the color whose density you want to adjust, and press .
2 | Select the desired density level, and press .
3 | Use / to adjust the density. Density adjustment Set a "+" value to increase the density. Set a "-" value to decrease the density. Example adjustment of each density area
<High> |
<Medium> |
<Low> |
4 | Press . If you want to also make adjustments on other density levels, repeat the operations in steps 2 to 4.

101K-072